IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "famous-mine-kumaushi-real-listing.ifc"
Time stamp: "2026-05-09T00:00:00"
Author: "BIM.HOUSE"
Organization: "Enabler Inc."
Preprocessor: "IFC4 Add2 — Real Listing AI Design"
Originating system: "BIM.HOUSE"
Application: "BIM.HOUSE" version "1.0" identifier "bim.house"

People and organizations
  Person (none given)
  Owner history of Person (none given) | application "BIM.HOUSE" version "1.0" identifier "bim.house" | change ADDED | created 1714000000 (2024-04-24T23:06:40Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "嶺 MINE — Eight Identical Cor-Ten Cubes on a Big Dipper (標茶町西熊牛原野 4線)" | long name "BIM.HOUSE" | phase "1-story ★ ONE typology / ONE material / ONE aperture / 8 floor levels ★ 8 棟 100% 同形 Cor-Ten 立方体 (7×7×4m) を 100m × 100m 山頂台地に北斗七星パターン散在 / 全面 Cor-Ten 6mm + SIPs t=245 (U=0.16, G3+, C=0.5) / 駒ヶ岳安山岩 600mm 石垣 plinth ring / ★ アイヌ刺繍 laser-cut Cor-Ten 1.5×3m aperture × 8 / skip-floor -2500〜+1500mm で 8 機能分節 / PV 72kW + LFP 30kWh + 地中熱 HP + KAGI lock + Face ID, 392sqm proposed for 5000sqm lot at 北海道川上郡標茶町西熊牛原野 4線 (Nishikumaushi-genya, 4sen, Shibecha-cho) — 標高 200m 小山頂上"
  IFCSITE "北海道川上郡標茶町西熊牛原野 4線 (Nishikumaushi-genya, 4sen, Shibecha-cho) — 標高 200m 小山頂上" | object type "Real listing site, 5000sqm" | elevation above sea level 0.
    IFCBUILDING "嶺 MINE — Eight Identical Cor-Ten Cubes on a Big Dipper (標茶町西熊牛原野 4線) (Proposed)" | object type "1F ★ ONE typology / ONE material / ONE aperture / 8 floor levels ★ 8 棟 100% 同形 Cor-Ten 立方体 (7×7×4m) を 100m × 100m 山頂台地に北斗七星パターン散在 / 全面 Cor-Ten 6mm + SIPs t=245 (U=0.16, G3+, C=0.5) / 駒ヶ岳安山岩 600mm 石垣 plinth ring / ★ アイヌ刺繍 laser-cut Cor-Ten 1.5×3m aperture × 8 / skip-floor -2500〜+1500mm で 8 機能分節 / PV 72kW + LFP 30kWh + 地中熱 HP + KAGI lock + Face ID 392sqm" | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "GF" | elevation 0.
        contains 161 elements
          1 x IFCSITE | names: "標茶町西熊牛原野 4線・200m 山頂台地" | material: "Generic" | property sets: Pset_BuildingElementCommon, BaseQuantities
          88 x IFCBUILDINGELEMENTPROXY | names: "Winter snow surface (typ. 1.2m)", "[DOJO α Dubhe] Komagatake andesite plinth ring", "[SHU β Merak] Komagatake andesite plinth ring" (+85 more) | material: "Generic"; "Natural Stone"; "Tree Trunk"; "Foliage" | property sets: Pset_BuildingElementCommon, BaseQuantities
          8 x IFCSLAB | FLOOR | names: "[DOJO α Dubhe] 床スラブ (+1500mm skip-floor)", "[SHU β Merak] 床スラブ (+600mm skip-floor)", "[KAKU γ Phecda] 床スラブ (+0mm skip-floor)" (+5 more) | material: "Reinforced Concrete" | property sets: Pset_SlabCommon, BaseQuantities
          32 x IFCWALL | names: "[DOJO α Dubhe] 北壁 (Cor-Ten 6mm + SIPs t=245 構造用 耐力壁 倍率 5.0)", "[DOJO α Dubhe] 南壁 (Cor-Ten 6mm + SIPs t=245 構造用 耐力壁 倍率 5.0) + 1.5×3m Ainu-motif laser-cut aperture", "[DOJO α Dubhe] 東壁 (Cor-Ten 6mm + SIPs t=245 構造用 耐力壁 倍率 5.0)" (+29 more) | material: "Generic" | property sets: Pset_WallCommon, BaseQuantities
          8 x IFCROOF | FLAT_ROOF | names: "[DOJO α Dubhe] 屋根 Cor-Ten flat t=6 (no eaves)", "[SHU β Merak] 屋根 Cor-Ten flat t=6 (no eaves)", "[KAKU γ Phecda] 屋根 Cor-Ten flat t=6 (no eaves)" (+5 more) | material: "Generic" | property sets: Pset_RoofCommon, BaseQuantities
          8 x IFCWINDOW | names: "[DOJO α Dubhe] ★ Ainu-motif aperture (laser-cut Cor-Ten 1.5×3m S)", "[SHU β Merak] ★ Ainu-motif aperture (laser-cut Cor-Ten 1.5×3m N)", "[KAKU γ Phecda] ★ Ainu-motif aperture (laser-cut Cor-Ten 1.5×3m N)" (+5 more) | material: "Generic" | property sets: Pset_WindowCommon, BaseQuantities
          8 x IFCDOOR | names: "[DOJO α Dubhe] 入口 (Cor-Ten 鋼扉 1.0×2.1m + KAGI スマートロック)", "[SHU β Merak] 入口 (Cor-Ten 鋼扉 1.0×2.1m + KAGI スマートロック)", "[KAKU γ Phecda] 入口 (Cor-Ten 鋼扉 1.0×2.1m + KAGI スマートロック)" (+5 more) | material: "Generic" | property sets: Pset_DoorCommon, BaseQuantities
          8 x IFCFURNISHINGELEMENT | names: "[DOJO α Dubhe] 内部装置: SJJJF 7×7 公式マット道場", "[SHU β Merak] 内部装置: 主屋: 書庫 + ベッド", "[KAKU γ Phecda] 内部装置: 客屋: 4 ベッド dorm" (+5 more) | material: "Tatami (Igusa)"; "Generic"; "Copper"; "Solid Wood" | property sets: Pset_BuildingElementCommon, BaseQuantities

Property sets
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCSITE)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "標茶町西熊牛原野 4線・200m 山頂台地" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Winter snow surface (typ. 1.2m)" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[DOJO α Dubhe] Komagatake andesite plinth ring" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[DOJO α Dubhe] 内部装置: SJJJF 7×7 公式マット道場" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[SHU β Merak] Komagatake andesite plinth ring" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[SHU β Merak] 内部装置: 主屋: 書庫 + ベッド" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[KAKU γ Phecda] Komagatake andesite plinth ring" (IFCLABEL)
  Pset_BuildingElementCommon | properties | on 1 object (1 IFCFURNISHINGELEMENT)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[KAKU γ Phecda] 内部装置: 客屋: 4 ベッド dorm" (IFCLABEL)
  Pset_BuildingElementCommon: 89 more contents on 89 objects not shown
  BaseQuantities | quantities | on 16 objects (16 IFCWALL)
    Height = 4.0000 [MILLI METRE]
    Length = 7.0000 [MILLI METRE]
    NetSideArea = 28.0000 [SQUARE_METRE]
    NetVolume = 5.6000 [CUBIC_METRE]
  BaseQuantities | quantities | on 16 objects (16 IFCWALL)
    Height = 4.0000 [MILLI METRE]
    Length = 0.2000 [MILLI METRE]
    NetSideArea = 0.8000 [SQUARE_METRE]
    NetVolume = 5.6000 [CUBIC_METRE]
  BaseQuantities | quantities | on 8 objects (8 IFCBUILDINGELEMENTPROXY)
    NetVolume = 48.6000 [CUBIC_METRE]
  BaseQuantities | quantities | on 8 objects (8 IFCSLAB)
    NetArea = 49.0000 [SQUARE_METRE]
    NetVolume = 9.8000 [CUBIC_METRE]
  BaseQuantities | quantities | on 8 objects (8 IFCROOF)
    NetArea = 49.0000 [SQUARE_METRE]
    NetVolume = 12.2500 [CUBIC_METRE]
  BaseQuantities | quantities | on 8 objects (8 IFCFURNISHINGELEMENT)
    NetVolume = 6.3000 [CUBIC_METRE]
  BaseQuantities | quantities | on 6 objects (6 IFCWINDOW)
    Area = 4.5000 [SQUARE_METRE]
    NetVolume = 0.9900 [CUBIC_METRE]
    OverallHeight = 3.0000 [MILLI METRE]
    OverallWidth = 1.5000 [MILLI METRE]
  BaseQuantities | quantities | on 6 objects (6 IFCDOOR)
    Area = 2.1000 [SQUARE_METRE]
    NetVolume = 0.4830 [CUBIC_METRE]
    OverallHeight = 2.1000 [MILLI METRE]
    OverallWidth = 1.0000 [MILLI METRE]
  BaseQuantities: 9 more contents on 13 objects not shown
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[DOJO α Dubhe] 床スラブ (+1500mm skip-floor)" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[SHU β Merak] 床スラブ (+600mm skip-floor)" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[KAKU γ Phecda] 床スラブ (+0mm skip-floor)" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[SHOKU δ Megrez] 床スラブ (+0mm skip-floor)" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[KAZOKU ε Alioth] 床スラブ (+0mm skip-floor)" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[YU ζ Mizar] 床スラブ (-2500mm skip-floor)" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[OTO η Alkaid] 床スラブ (-500mm skip-floor)" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[SHI Polaris] 床スラブ (-1500mm skip-floor)" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "[DOJO α Dubhe] 北壁 (Cor-Ten 6mm + SIPs t=245 構造用 耐力壁 倍率 5.0)" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "[DOJO α Dubhe] 南壁 (Cor-Ten 6mm + SIPs t=245 構造用 耐力壁 倍率 5.0) + 1.5×3m Ainu-motif laser-cut aperture" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "[DOJO α Dubhe] 東壁 (Cor-Ten 6mm + SIPs t=245 構造用 耐力壁 倍率 5.0)" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "[DOJO α Dubhe] 西壁 (Cor-Ten 6mm + SIPs t=245 構造用 耐力壁 倍率 5.0)" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "[SHU β Merak] 北壁 (Cor-Ten 6mm + SIPs t=245 構造用 耐力壁 倍率 5.0) + 1.5×3m Ainu-motif laser-cut aperture" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "[SHU β Merak] 南壁 (Cor-Ten 6mm + SIPs t=245 構造用 耐力壁 倍率 5.0)" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "[SHU β Merak] 東壁 (Cor-Ten 6mm + SIPs t=245 構造用 耐力壁 倍率 5.0)" (IFCLABEL)
  Pset_WallCommon | properties | on 1 object (1 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "[SHU β Merak] 西壁 (Cor-Ten 6mm + SIPs t=245 構造用 耐力壁 倍率 5.0)" (IFCLABEL)
  Pset_WallCommon: 24 more contents on 24 objects not shown
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 49.00 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "[DOJO α Dubhe] 屋根 Cor-Ten flat t=6 (no eaves)" (IFCLABEL)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 49.00 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "[SHU β Merak] 屋根 Cor-Ten flat t=6 (no eaves)" (IFCLABEL)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 49.00 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "[KAKU γ Phecda] 屋根 Cor-Ten flat t=6 (no eaves)" (IFCLABEL)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 49.00 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "[SHOKU δ Megrez] 屋根 Cor-Ten flat t=6 (no eaves)" (IFCLABEL)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 49.00 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "[KAZOKU ε Alioth] 屋根 Cor-Ten flat t=6 (no eaves)" (IFCLABEL)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 49.00 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "[YU ζ Mizar] 屋根 Cor-Ten flat t=6 (no eaves)" (IFCLABEL)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 49.00 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "[OTO η Alkaid] 屋根 Cor-Ten flat t=6 (no eaves)" (IFCLABEL)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 49.00 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "[SHI Polaris] 屋根 Cor-Ten flat t=6 (no eaves)" (IFCLABEL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "[DOJO α Dubhe] ★ Ainu-motif aperture (laser-cut Cor-Ten 1.5×3m S)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "[SHU β Merak] ★ Ainu-motif aperture (laser-cut Cor-Ten 1.5×3m N)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "[KAKU γ Phecda] ★ Ainu-motif aperture (laser-cut Cor-Ten 1.5×3m N)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "[SHOKU δ Megrez] ★ Ainu-motif aperture (laser-cut Cor-Ten 1.5×3m S)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "[KAZOKU ε Alioth] ★ Ainu-motif aperture (laser-cut Cor-Ten 1.5×3m S)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "[YU ζ Mizar] ★ Ainu-motif aperture (laser-cut Cor-Ten 1.5×3m S)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "[OTO η Alkaid] ★ Ainu-motif aperture (laser-cut Cor-Ten 1.5×3m E)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "[SHI Polaris] ★ Ainu-motif aperture (laser-cut Cor-Ten 1.5×3m W)" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "Rw 35dB" (IFCLABEL)
    FireRating = "30" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[DOJO α Dubhe] 入口 (Cor-Ten 鋼扉 1.0×2.1m + KAGI スマートロック)" (IFCLABEL)
    ThermalTransmittance = 1.8 (IFCREAL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "Rw 35dB" (IFCLABEL)
    FireRating = "30" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[SHU β Merak] 入口 (Cor-Ten 鋼扉 1.0×2.1m + KAGI スマートロック)" (IFCLABEL)
    ThermalTransmittance = 1.8 (IFCREAL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "Rw 35dB" (IFCLABEL)
    FireRating = "30" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[KAKU γ Phecda] 入口 (Cor-Ten 鋼扉 1.0×2.1m + KAGI スマートロック)" (IFCLABEL)
    ThermalTransmittance = 1.8 (IFCREAL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "Rw 35dB" (IFCLABEL)
    FireRating = "30" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[SHOKU δ Megrez] 入口 (Cor-Ten 鋼扉 1.0×2.1m + KAGI スマートロック)" (IFCLABEL)
    ThermalTransmittance = 1.8 (IFCREAL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "Rw 35dB" (IFCLABEL)
    FireRating = "30" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[KAZOKU ε Alioth] 入口 (Cor-Ten 鋼扉 1.0×2.1m + KAGI スマートロック)" (IFCLABEL)
    ThermalTransmittance = 1.8 (IFCREAL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "Rw 35dB" (IFCLABEL)
    FireRating = "30" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[YU ζ Mizar] 入口 (Cor-Ten 鋼扉 1.0×2.1m + KAGI スマートロック)" (IFCLABEL)
    ThermalTransmittance = 1.8 (IFCREAL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "Rw 35dB" (IFCLABEL)
    FireRating = "30" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[OTO η Alkaid] 入口 (Cor-Ten 鋼扉 1.0×2.1m + KAGI スマートロック)" (IFCLABEL)
    ThermalTransmittance = 1.8 (IFCREAL)
  Pset_DoorCommon | properties | on 1 object (1 IFCDOOR)
    AcousticRating = "Rw 35dB" (IFCLABEL)
    FireRating = "30" (IFCLABEL)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "[SHI Polaris] 入口 (Cor-Ten 鋼扉 1.0×2.1m + KAGI スマートロック)" (IFCLABEL)
    ThermalTransmittance = 1.8 (IFCREAL)