IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "u-5100sips-42qah7zy-real-listing.ifc"
Time stamp: "2026-05-09T00:00:00"
Author: "BIM.HOUSE"
Organization: "Enabler Inc."
Preprocessor: "IFC4 Add2 — Real Listing AI Design"
Originating system: "BIM.HOUSE"
Application: "BIM.HOUSE" version "1.0" identifier "bim.house"

People and organizations
  Person (none given)
  Owner history of Person (none given) | application "BIM.HOUSE" version "1.0" identifier "bim.house" | change ADDED | created 1714000000 (2024-04-24T23:06:40Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN

Spatial structure
IFCPROJECT "カタログの家 — 5軸100点モデル (籾殻SIPs)" | long name "BIM.HOUSE" | phase "2-story 籾殻SIPs・杉CLT 陸屋根 杉板外装 (SOLUNA), 196sqm proposed for 500sqm lot at 想定敷地 500㎡"
  IFCSITE "想定敷地 500㎡" | object type "Real listing site, 500sqm" | elevation above sea level 0.
    IFCBUILDING "カタログの家 — 5軸100点モデル (籾殻SIPs) (Proposed)" | object type "2F 籾殻SIPs・杉CLT 陸屋根 杉板外装 (SOLUNA) 196sqm" | reference height above sea level 0. | terrain above sea level 0.
      IFCBUILDINGSTOREY "GF" | elevation 0.
        contains 50 elements
          6 x IFCSLAB | FLOOR | names: "基礎スラブ (布基礎)", "1F 床 LDK", "1F 床 個室棟" (+3 more) | material: "Generic" | property sets: Pset_SlabCommon, BaseQuantities
          3 x IFCROOF | FLAT_ROOF | names: "主屋根 (ガルバ立平)", "越屋根 (ハイサイドライト)", "太陽光パネル PV 6kW" | material: "Generic" | property sets: Pset_RoofCommon, BaseQuantities
          18 x IFCWALL | names: "外壁 南面 耐力壁", "外壁 北面 耐力壁", "外壁 西面 耐力壁" (+12 more) | material: "Generic" | property sets: Pset_WallCommon, BaseQuantities
          19 x IFCWINDOW | names: "南面窓 1F-1", "南面窓 1F-2", "南面窓 1F-3" (+16 more) | material: "Generic" | property sets: Pset_WindowCommon, BaseQuantities
          4 x IFCSPACE | INTERNAL | names: "吹抜 (LDK上部)", "ピアノ室", "雨水タンク 300L" (+1 more) | material: "Generic" | property sets: Pset_SpaceCommon, BaseQuantities

Property sets
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "基礎スラブ (布基礎)" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1F 床 LDK" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1F 床 個室棟" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "1F 床 水回り" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "2F 床" (IFCLABEL)
  Pset_SlabCommon | properties | on 1 object (1 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "ロフト床" (IFCLABEL)
  BaseQuantities | quantities | on 12 objects (12 IFCWINDOW)
    Area = 3.2560 [SQUARE_METRE]
    NetVolume = 0.6512 [CUBIC_METRE]
    OverallHeight = 2.2000 [MILLI METRE]
    OverallWidth = 1.4800 [MILLI METRE]
  BaseQuantities | quantities | on 6 objects (6 IFCWALL)
    Height = 2.9000 [MILLI METRE]
    Length = 3.3730 [MILLI METRE]
    NetSideArea = 9.7817 [SQUARE_METRE]
    NetVolume = 1.4673 [CUBIC_METRE]
  BaseQuantities | quantities | on 5 objects (5 IFCWINDOW)
    Area = 0.5950 [SQUARE_METRE]
    NetVolume = 0.1190 [CUBIC_METRE]
    OverallHeight = 0.3500 [MILLI METRE]
    OverallWidth = 1.7000 [MILLI METRE]
  BaseQuantities | quantities | on 4 objects (4 IFCWALL)
    Height = 2.9000 [MILLI METRE]
    Length = 9.8000 [MILLI METRE]
    NetSideArea = 28.4200 [SQUARE_METRE]
    NetVolume = 5.6840 [CUBIC_METRE]
  BaseQuantities | quantities | on 4 objects (4 IFCWALL)
    Height = 2.9000 [MILLI METRE]
    Length = 0.2000 [MILLI METRE]
    NetSideArea = 0.5800 [SQUARE_METRE]
    NetVolume = 5.8000 [CUBIC_METRE]
  BaseQuantities | quantities | on 4 objects (4 IFCWALL)
    Height = 2.9000 [MILLI METRE]
    Length = 0.1500 [MILLI METRE]
    NetSideArea = 0.4350 [SQUARE_METRE]
    NetVolume = 1.4673 [CUBIC_METRE]
  BaseQuantities | quantities | on 2 objects (2 IFCSLAB)
    NetArea = 25.0000 [SQUARE_METRE]
    NetVolume = 4.5000 [CUBIC_METRE]
  BaseQuantities | quantities | on 2 objects (2 IFCWINDOW)
    Area = 8.1600 [SQUARE_METRE]
    NetVolume = 1.6320 [CUBIC_METRE]
    OverallHeight = 2.4000 [MILLI METRE]
    OverallWidth = 3.4000 [MILLI METRE]
  BaseQuantities: 11 more contents on 11 objects not shown
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 98.00 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "主屋根 (ガルバ立平)" (IFCLABEL)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 9.00 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "越屋根 (ハイサイドライト)" (IFCLABEL)
  Pset_RoofCommon | properties | on 1 object (1 IFCROOF)
    IsExternal = TRUE (IFCBOOLEAN)
    ProjectedArea = 90.24 (IFCAREAMEASURE) [SQUARE_METRE]
    Reference = "太陽光パネル PV 6kW" (IFCLABEL)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "外壁 南面 耐力壁" (IFCLABEL)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "外壁 北面 耐力壁" (IFCLABEL)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "外壁 西面 耐力壁" (IFCLABEL)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "外壁 東面 耐力壁" (IFCLABEL)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "間仕切 耐力壁X-S" (IFCLABEL)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "間仕切 耐力壁X-N" (IFCLABEL)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "間仕切 耐力壁Y-W" (IFCLABEL)
  Pset_WallCommon | properties | on 2 objects (2 IFCWALL)
    FireRating = "30" (IFCLABEL)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
    Reference = "間仕切 耐力壁Y-E" (IFCLABEL)
  Pset_WallCommon: 1 more content on 2 objects not shown
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "南面窓 1F-1" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "南面窓 1F-2" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "南面窓 1F-3" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "南面窓 1F-4" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "南面窓 1F-5" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "南面窓 1F-6" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "南面窓 2F-1" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    GlazingAreaFraction = 0.85 (IFCREAL)
    IsExternal = TRUE (IFCBOOLEAN)
    Reference = "南面窓 2F-2" (IFCLABEL)
    ThermalTransmittance = 2.1 (IFCREAL)
  Pset_WindowCommon: 11 more contents on 11 objects not shown
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    GrossPlannedArea = 10.24 (IFCAREAMEASURE) [SQUARE_METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    PubliclyAccessible = FALSE (IFCBOOLEAN)
    Reference = "吹抜 (LDK上部)" (IFCLABEL)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    GrossPlannedArea = 8.10 (IFCAREAMEASURE) [SQUARE_METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    PubliclyAccessible = FALSE (IFCBOOLEAN)
    Reference = "ピアノ室" (IFCLABEL)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    GrossPlannedArea = 0.64 (IFCAREAMEASURE) [SQUARE_METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    PubliclyAccessible = FALSE (IFCBOOLEAN)
    Reference = "雨水タンク 300L" (IFCLABEL)
  Pset_SpaceCommon | properties | on 1 object (1 IFCSPACE)
    GrossPlannedArea = 12.74 (IFCAREAMEASURE) [SQUARE_METRE]
    IsExternal = FALSE (IFCBOOLEAN)
    PubliclyAccessible = FALSE (IFCBOOLEAN)
    Reference = "縁側 デッキ (南濡れ縁)" (IFCLABEL)